#AP6255_NVRAM_V1.1.7_20180516.txt
# Cloned from bcm94345wlpagb_p2xx.txt 
NVRAMRev=$Rev: 498373 $
sromrev=11
vendid=0x14e4
devid=0x43ab
manfid=0x2d0
prodid=0x06e4
macaddr=00:90:4c:c5:12:38
nocrc=1
boardtype=0x6e4
boardrev=0x1304
#XTAL 37.4MHz
xtalfreq=37400
btc_mode=1
#-----------------------------------------
#boardflags: 5GHz eTR switch by default
#            2.4GHz eTR switch by default
#            bit1 for btcoex
boardflags=0x00480201
boardflags2=0x40800000
boardflags3=0x48200100
phycal_tempdelta=15
rxchain=1
txchain=1
aa2g=1
aa5g=1
tssipos5g=1
tssipos2g=1
femctrl=0
AvVmid_c0=1,165,2,100,2,100,2,100,2,100
pa2ga0=-195,5558,-672
pa2ga1=-118,4850,-635
pa5ga0=-201,6184,-750,-190,6351,-762,-194,6137,-743,-184,6220,-746
pa5ga1=-142,4930,-655,-150,4859,-646,-156,4887,-644,-158,4864,-641
itrsw=1
pdoffset2g40ma0=10
pdoffset40ma0=0xaaaa
pdoffset80ma0=0xaaaa
extpagain5g=2
extpagain2g=2
tworangetssi2g=0
tworangetssi5g=0
# LTECX flags
# WCI2
ltecxmux=0
ltecxpadnum=0x0504
ltecxfnsel=0x22
ltecxgcigpio=0x32

maxp2ga0=70
cckbw202gpo=0x2210
cckbw20ul2gpo=0x2200
ofdmlrbw202gpo=0x0000
dot11agofdmhrbw202gpo=0x2222
mcsbw202gpo=0x98422200
mcsbw402gpo=0x98777755

maxp5ga0=76,72,72,72
mcsbw205glpo=0xb7544322
mcsbw205gmpo=0xb7533422
mcsbw205ghpo=0xb8644422
mcsbw405glpo=0xa6543311
mcsbw405gmpo=0xb7433311
mcsbw405ghpo=0xd9754432
mcsbw805glpo=0xd8532211
mcsbw805gmpo=0xc7422200
mcsbw805ghpo=0xd9744432

swctrlmap_2g=0x00000000,0x00000000,0x00000000,0x010000,0x3ff
swctrlmap_5g=0x00100010,0x00200020,0x00200020,0x010000,0x3fe
swctrlmapext_5g=0x00000000,0x00000000,0x00000000,0x000000,0x3
swctrlmapext_2g=0x00000000,0x00000000,0x00000000,0x000000,0x3
vcodivmode=1
deadman_to=481500000
#ed_thresh2g=-54
#ed_thresh5g=-54
#eu_edthresh2g=-54
#eu_edthresh5g=-54
ed_thresh2g=-69
ed_thresh5g=-69
eu_edthresh2g=-69
eu_edthresh5g=-69
ldo1=4
rawtempsense=0x1ff
cckPwrIdxCorr=3
cckTssiDelay=150
ofdmTssiDelay=150
txpwr2gAdcScale=1
txpwr5gAdcScale=1
dot11b_opts=0x3aa85
cbfilttype=0
fdss_level_2g=4
fdss_level_5g=4
muxenab=0x10
